**ADA Accessibility Reqs. PD 605.1 [Form 464 Ref. Removed]**

Completion of Form 464, Design Exception Variance Request is required when the controlling design criteria as detailed in Form 463, Design Data are not met. While important, ADA curb ramp design criteria requirements are not part of the controlling design criteria as defined in the Federal Register. PD 605.1 “ADA Accessibility Requirements in CDOT Transportation Projects” previously referenced Form 464, Design Exception Variance Request as a temporary part of the ADA curb ramp variance documentation process while the separate ADA Curb Ramp Variance Support Document was finalized.

The ADA Curb Ramp Variance Support Document now fully addresses a wide spectrum of potential ADA curb ramp variance scenarios. As a result, references to Form 464 have been removed from PD 605.1. Controlling criteria for curb ramps should be Standard Plan M-608-1 Curb Ramps and the PROWAG.

If you have any questions or comments, please contact Joshua Keith at 303-757-9021.

**Resources:**

PD 605.1 “ADA Accessibility Requirements in CDOT Transportation Projects”:

<https://www.codot.gov/business/civilrights/ada/assets/0605-1.pdf>

ADA Curb Ramp Variance Support Document:

<https://www.codot.gov/business/civilrights/ada/assets/curb-ramp-variance-support-document-091917-final.pdf>

Form 463:

<https://www.codot.gov/library/forms/cdot0463.pdf>