<sample project special> 603624dp

<date> 10/23/2013

1

REVISION OF SECTIONS 603, 624, 705AND 712

DRAINAGE PIPE

Sections 603, 624, 705and 712 of the Standard Specifications are hereby revised for this project as follows:

Subsection 603.07 shall include the following:

Joint systems for siphons, irrigation systems, and storm drains shall be watertight.

Subsection 603.07(c) shall include the following:

Watertight joint systems for plastic pipe shall conform to subsection 705.03.

In subsection 624.02, delete the last line in the table of the first paragraph and replace with the following:

**Abbreviation Description Subsection**

Plastic Polyvinyl Chloride (PVC), Polyethylene (PE)

and Polypropylene (PP) 712.13

In subsection 624.02 delete the third paragraph and replace it with the following:

Connecting bands shall receive the same corrosion protection as the pipe with which they are used. Coatings conforming to the requirements of Sections 706 and 707 will be permitted as applicable. Connecting bands and pipe extensions shall be of similar metal, or of non-metallic material, to avoid galvanic corrosion.

End sections for concrete or metal pipe shall be the same material as the pipe and meet the requirements for the same class as that specified for the pipe in accordance with Table 624-1.

Plastic end sections shall not be used. When plastic pipe is to be installed with end sections, steel or concrete end sections meeting the same class as that specified for the pipe in accordance with Table 624-1 shall be used.

In subsection 624.02 delete the fourth paragraph and replace it with the following:

The Contractor may furnish any pipe material allowed in Table 624-1 for the class of pipe specified in the Contract except for storm drains. The Contractor may furnish RCP, PVC or PP allowed in Table 624-1 for the class of pipe specified in the Contract for storm drains. The Contractor shall state at the preconstruction conference the pipe materials intended to be furnished.

2

REVISION OF SECTIONS 603, 624, 705, AND 712

DRAINAGE PIPE

In subsection 624.02 delete Table 624-1 and replace it with the following:

**TABLE 624-1**

**Materials Allowed for Class of Pipe**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Material Allowed\*\*** | **Class of Pipe\*** | | | | | | | | | | |
| **0** | **1** | **2** | **3** | **4** | **5** | **6**4 | **7** | **8** | **9** | **10**4 |
| CSP | Y | N | N | N | N | N | N | N | N | N | N |
| Bit. Co. CSP | Y | Y1 | N | N | N | N | N | N | N | N | N |
| A.F. Bo. CSP | Y | Y | Y | Y | Y | Y | Y | N | N | N | N |
| CAP | Y | Y2 | Y2 | Y2 | Y2 | Y | N | N | N | N | N |
| PCSP - both sides | Y | Y | Y | Y | Y | Y | Y | N | N | N | N |
| PVC6 | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
| PE6 | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
| PP6 | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
| RCP (SP0)3,5 | Y | Y | N | N | N | N | N | Y | N | N | N |
| RCP (SP1)3,5 | Y | Y | Y | N | N | N | N | Y | Y | N | N |
| RCP (SP2)3,5 | Y | Y | Y | Y | Y | N | N | Y | Y | Y | N |
| RCP (SP3)3,5 | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y | Y |
| \* As determined by the Department in accordance with the CDOT *Pipe Selection Guide*. Determination is based on abrasion and corrosion resistance.  \*\* Y=Yes; N=No.  1 Coated Steel Structural Plate Pipe of equal or greater diameter, conforming to Section 510, may be substituted for Bit. Co. CSP at no additional cost to the project.  2 Aluminum Alloy Structural Plate Pipe of equal or greater diameter, conforming to Section 510, may be substituted for CAP at no additional cost to the project.  3 SP= Class of Sulfate Protection required in accordance with subsection 601.04 as revised for this project. RCP shall be manufactured using the cementitious material required to meet the SP class specified.  4 For pipe classes 6 and 10, the RCP shall be coated in accordance with subsection 706.07 when the pH of either the soil or water is less than 5. The Contract will specify when RCP is to be coated.  5 Concrete shall have a compressive strength of 4500 psi or greater.  6 In accordance with subsection 712.13. | | | | | | | | | | | |

3

REVISION OF SECTIONS 603, 624, 705, 707 AND 712

DRAINAGE PIPE

Subsection 624.03 shall include the following:

Joint systems for siphons, irrigation systems, and storm drains shall be watertight. Watertight joint systems for plastic pipe shall conform to subsection 705.03.

Subsection 705.03 shall include the following:

Watertight joint systems for plastic pipe shall be in accordance with ASTM D3212.

In subsection 712.13 (b), delete (1) and (2) and replace with the following:

(1) AASHTO M 304 (Profile) for nominal pipe sizes of 4 to 36 inches.

(2) ASTM F794 (Profile) for nominal pipe sizes 4 to 36 inches with 46 psi minimum pipe stiffness

Add subsection 712.13(c) as follows:

*(c) Polypropylene (PP) Pipe*

1. AASHTO M 330 for nominal pipe sizes of 12 to 60 inches (300 to 1500 mm) with the following exceptions:
   1. Type S and Type SP are acceptable (Type C, Type CP and Type D will not be accepted).