

Standards and Specifications Unit

**Memorandum**

**DATE**: May 12, 2016

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Sections 202, 627 and 708 Pavement Marking Paint

Effective this date, our unit is issuing a revised version of standard special provision, Revision of Sections 202, 627 and 708 Pavement Marking Paint. This revised standard special provision is 3 pages long and replaces a standard special provision having the title, Revision of Sections 627 and 708 Pavement Marking Paint dated January 31, 2013.

Use this revised standard special provision in projects having pavement marking paint, except for chip seal projects, beginning with projects advertised on or after June 9, 2016. You are free to use this standard special provision in projects advertised before this date.

This revisions contained in this version defines the requirements for removing temporary pavement marking from both the final alignment and transitions. It removes sandblasting as a method for removing pavement marking, and also removes waterborne paint as an option for pavement marking paint.

Those of you who keep a book of Standard Special Provisions should replace the now obsolete standard special provision with this revised version. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/2011-construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “Recently Issued Special Provisions”.

If you have any questions or comments, please contact this office.