July 3, 2017

REVISION OF SECTION 208

EROSION CONTROL

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction*. It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Projects with anticipated disturbance of under one acre.

Section 208 of the Standard Specifications is hereby revised for this project as follows:

In subsection 208.03(c) delete the first paragraph and replace it with the following

*Erosion Control Management (ECM).* Erosion Control Management for this project shall consist of Erosion Control Inspection and the SWMP Administration. All ECM staff shall have working knowledge and experience in construction, and shall have successfully completed the Transportation Erosion Control Supervisory Certificate Training (TECS) as provided by the Department. The Superintendent will not be permitted to serve in an ECM role. The Erosion Control Inspector (ECI) and the SWMP Administrator may be the same person in projects involving less than 40 acres of disturbed area.

In subsection 208.03(c)1 delete the first paragraph and replace it with the following:

SWMP Administration. The SWMP shall be maintained by a SWMP Administrator. In the case of a project requiring only one TECS, the SWMP Administrator may also be the ECI for the project. The name of the SWMP Administrator shall be recorded on the SWMP Section 3. B. The SWMP Administrator shall have full responsibility to maintain and update the SWMP and identify to the Superintendent critical action items needed to conform to the CDPS-SCP as follows:

In subsection 208.03(c)2 delete the first paragraph and replace It with the following:

One ECI is required for every 40 acres of total disturbed area which is currently receiving temporary and interim stabilization measures as defined in subsection 208.04 (e). An ECI shall not be responsible for more than 40 acres in the project. Accepted permanent stabilization methods as defined in subsection 208.04 (e) will not be included in the 40 acres.

In subsection 208.03(d)1 delete item (1) and replace it with the following:

1. SWMP Site Maps and Plan Title Sheet *-* Construction site boundaries, ground surface disturbance, limits of cut and fill, flow arrows, structural BMPs, non-structural BMPs, Springs, Streams, Wetlands and surface water. Also included on the sheets is the protection of trees, shrubs and cultural resources.

In subsection 208.05(n), in the list of requirements for pre-fabricated concrete washout structures, delete item (2) and replace it with the following:

1. Structure shall be located 50 horizontal feet away from State waters, and shall be confined so that no potential pollutants will enter State waters and other sensitive areas are as defined in the Contract. Locations shall be as approved by the Engineer. The site shall signed as “Concrete Washout”.

In subsection 208.11 delete the first paragraph and replace it with the following:

Erosion Control Management will be measured as the actual number of days of ECM work performed, regardless of the number of personnel required for SWMP Administration and Erosion Control Inspection, including erosion control inspections, documentation, meeting participation, SWMP Administration, and the preparation of the SWMP notebook. If the combined hours of SWMP Administration and Erosion Control Inspection is four hours or less in a day, the work will be measured as ½ day. If the combined hours of SWMP Administration and Erosion Control Inspection is more than four hours in a day, the work will be measured as one day. Total combined hours of ECM work exceeding eight hours in a day will still be paid as one day.