1

REVISION OF SECTION 412  
PCCP SHOULDER JOINTS

Section 412 of the Standard Specifications is hereby revised for this project as follows:

Subsection 412.13(b)2 shall include the following:

Transverse weakened plane joints on the shoulder shall not require the placement of dowels on © joints as shown on Standard Plan M-412-1.

=============================================================================

Instructions to the designer:

Include this project special provision on projects with shoulders less than 8 feet wide and where the Region does not have plans to add a future driving lane or bus lane on the shoulder.  
  
Use of this Project Special Provision shall be approved by the Region Materials Engineer.