Sample project special: 607wsf

02-03-11 (Re-issued 07-03-17)

REVISION OF SECTIONS 607 AND 710

WOOD SNOW FENCE

Section 607 of the Standard Specifications is hereby revised for this project as follows:

Subsection 607.02 shall include the following:

Timber for wood snow fence panels shall conform to subsection 710.041

Subsection 607.04 shall include the following:

Wood snow fence will be measured by the actual number of 12-foot long panels that are installed and accepted.

Subsection 607.05 shall include the following:

**Pay Item** **Pay Unit**

Wood Snow Fence (\_\_ Foot High) Each

Payment for wood snow fence will be full compensation for all labor, materials and equipment required to complete the work, including panels, slats, hardware, and all other items that are incidental to the construction of the fence.

Add subsection 710.041 as follows:

**710.041 Wood Snow Fence.** Timber for wood snow fence panels shall conform to the requirements of ASTM F 537.