Sample Project Special Provision: 630pba

Issued: December 7, 2017

REVISION OF SECTION 630  
PEDESTRIAN BARRICADE (ADA)

Section 630 of the Standard Specifications is hereby revised for this project as follows:

Subsection 630.01 shall include the following:

This work consists of the construction of temporary pedestrian barricades which are fully ADA compliant.

Subsection 630.02 shall include the following:

The pedestrian barricade shall conform to MUTCD 6F.71 for pedestrian traffic control. The barricade shall be made of High Density Polyethylene (HDPE) with Ultraviolet (UV) stabilizers, or other approved material. It shall be able to interlock with adjacent barricades of the same product such that it forms a wall or a rail.

The pedestrian barricade shall comply with the crash test requirements contained in NCHRP Report 350 (only applicable for pedestrian barricades developed prior to 2011) or MASH Level TL3.

The pedestrian barricade shall have a continuous detectable bottom and top surface to be detectable to users of long canes. The bottom of barricade shall be no more than 2 inches above the ground. The top of barricade shall be no lower than 32 inches above the ground. The gap to the bottom of the barricade may be used for drainage. The barricade shall be reflectorized in accordance with subsection 630.02. No extended bases or protrusions shall extend into the walkway.

The Contractor shall submit manufacturer’s documentation confirming that the barricade meets all applicable ADA requirements for barricades or rail.

Subsection 630.13 shall include the following:

Placement of the Pedestrian Barricade (ADA) shall be in accordance with manufacturer recommendations.

The ADA pedestrian barricade may be moved to other locations as shown on the plans or as directed upon completion of use at one location.

In subsection 630.15, delete the third paragraph and replace with the following:

Traffic channelizing devices consisting of vertical panels, traffic cones, or drum channelizing devices will be measured by the unit. Concrete barriers will be measured by the linear foot. Barricades will be measured by the number used, except Pedestrian Barricade (ADA). Barricade warning lights shall be furnished as a part of this item when required by the Traffic Control Plan (TCP). Advance Warning Flashing or Sequencing Arrow Panels will be measured by the unit according to size.

Pedestrian Barricade (ADA) will be measured as the actual linear feet of barricade installed and accepted.

Subsection 630.16 shall include the following:

Payment will be made under:

**Pay Item Pay Unit**

Pedestrian Barricade (ADA) Linear Foot

Movement of the Pedestrian Barricade (ADA) to different locations, when required, will not be measured and paid for separately, but shall be included in the work.