

Standards and Specifications Unit

**Memorandum**

**DATE**: December 28, 2017

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Sections 206 and 703, Structure Backfill (Flow-Fill)

Effective this date, our unit is issuing a revised version of standard special provision, Revision of Sections 206 and 703, Structure Backfill (Flow-Fill). This revised standard special provision is 1 page long and replaces a standard special provision having the title, Revision of Section 206, Structure Backfill (Flow-Fill) dated July 3, 2017.

Use this revised standard special provision in projects having Structure Backfill, beginning with projects advertised on or after January 25, 2018. You are free to use this standard special provision in projects advertised before this date.

The revisions contained in this version allow for the use of Structure Backfill (Class 3) as backfill for culverts and sewer pipes, and defines the requirements for this class.

Those of you who keep a book of Standard Special Provisions should replace the now obsolete standard special provision with this revised version. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/cdot-construction-specifications/2017-construction-standard-specs>

Please scroll down and visit the hyperlink, “[Recently Issued Special Provisions](https://www.codot.gov/business/designsupport/cdot-construction-specifications/2017-construction-standard-specs/recently-issued-special-provisions)”.

If you have any questions or comments, please contact this office.