Revise Section 601 of the Standard Specifications for this project as follows:

Revise Subsection 601.05, second paragraph as follows:

1. For air entrained concrete, the SAM number according to AASHTO TP118 Characterization of the Air-Void System of Freshly Mixed Concrete by the Sequential Pressure Method (Super Air Meter) shall be reported. The SAM meter readings for each step shall be included. . A SAM leak test shall be performed prior to the SAM testing. Results of the leak test shall be included in the SAM data.