Date Issued 10.17.24

**Page 202-12, the fifth paragraph under the subsection, an incorrect reference.**

Smoothness for this project will be measured by the Department per subsection ~~105.08~~ 105.07. The MRI after grinding for each 0.10-mile section or fraction thereof shall have an MRI of 95 in/mile or less. Sections with an MRI greater than 95 in/mile shall be corrected by further diamond grinding.