Sample Project Special Provision: 608crt

Issued: 12/07/2017

REVISION OF SECTION 608  
 CURB RAMP (TEMPORARY)

Section 608 of the Standard Specifications is hereby revised for this project as follows:

Subsection 608.01 shall include the following:

This work consists of the construction of a temporary curb ramp which is fully ADA compliant at locations as shown on the plans.

Subsection 608.02 shall include the following:

The temporary curb ramp shall be made of an approved durable material coated with a slip-resistant surface. The width of the ramp shall be a minimum of 48 inches, and when required, a landing shall be attached. The slope of the ramp shall be no more than 1V:12H. The ramp shall accommodate a minimum weight of 800 pounds.

Protective edging shall be installed on both sides of the ramp when the drop is 3 inches or more. Edging shall be continuous and a minimum of 6 inches high.

Subsection 608.03 shall include the following:

1. *Curb Ramp (Temporary).* Construction and installation of the ramp shall be in accordance with the Plans.

The ramp shall be installed either perpendicular or parallel to the curb. When the ramp is installed parallel to the curb of the roadway, a 48-inch by 48-inch landing shall be constructed of the same material at the top of the ramp.

The ramp may be moved to other locations as shown on the plans or as directed upon completion of use at one location.

Subsection 608.05 shall include the following:

Curb Ramp (Temporary) will be measured as the actual number installed and accepted.

Subsection 608.06 shall include the following:

Payment will be made under:

**Pay Item Pay Unit**

Curb Ramp (Temporary) (Perpendicular) Each  
 Curb Ramp (Temporary) (Parallel) Each

Movement of the temporary curb ramp to different locations, when required, will not be measured and paid for separately, but shall be included in the work.