# Revise Section 401 of the Standard Specifications as follows:

## Revise Subsection 401.10, eighth paragraph, of the Standard Specifications as shown:

The following specific requirements shall apply to the identified asphalt pavers:

1. Blaw-Knox asphalt pavers manufactured prior to 2007 shall be equipped with the Blaw-Knox Materials Management Kit (MMK).
2. Cedarapids asphalt pavers shall be those that were manufactured in 1989 or later.
3. Caterpillar asphalt pavers manufactured prior to 2007 shall be equipped with deflector plates as identified in the December 2000 Service Magazine entitled “New Asphalt Deflector Kit {6630, 6631, 6640}”.