**CDOT’s 2019 Field Materials Manual**

**CP-52 Contractor Asphalt Mix Design Approval Procedures**

This materials bulletin replaces CP-52 of the *2019 Field Materials Manual.*  The RAP aggregate bulk specific gravity will be back-calculated using an assumed average aggregate water absorption of 1.01%. The corresponding assumed aggregate asphalt absorption will be 0.61. The corresponding CDOT Form # 429 has also been updated.

It is your responsibility as the owner of your *2019 Field Materials Manual* to print these pages for replacement within your printed copy of the manual. If you have questions, please contact Michael Stanford at 303-398-6576.



**References:**

All Material Bulletins can be found here: [Materials Bulletins](http://www.coloradodot.info/business/designsupport/materials-and-geotechnical/materials-bulletins).