# Revision of Section 208

# Silt Fence (Reinforced) (Special)

**Revise Section 208 of the Standard Specifications for this project as follows:**

Delete the second paragraph in Subsection 208.02 (b) and replace it with the following:

The geotextile of Silt Fence and Silt Fence (Reinforced) (Special) shall adhere to the following requirements:

Delete the first two sentences in Subsection 208.04 (c), and replace them with the following:

*Work Outside of the Right of Way.* Disturbed areas located outside the CDOT ROW are the Contractor’s responsibility, including staging areas and easements acquired by CDOT for construction.

Delete the sixth paragraph of Subsection 208.04 (f), and replace it with the following:

 Do not remove temporary BMP’s upon completion of this project.

Delete Subsection 208.05 (c), and replace it with the following:

*(c) Silt Fence and Silt Fence (Reinforced) (Special).* Install Silt Fence and Silt Fence (Reinforced) (Special) before grubbing or grading. Before placing Silt Fence (Reinforced) (Special), grade the ground to ensure the barrier sits on a level surface. Inspect the fence weekly to ensure the fence remains upright and excessive ponding does not occur. Where ponding occurs, direct water back into the ground via sediment trap or pump out to other areas. Do not discharge water directly into streams.

In Subsection 208.11, delete the second paragraph and replace it with the following:

Measure Silt fence and Silt Fence (Reinforced) (Special), silt berms, erosion logs, gravel bags, silt dikes, temporary berms, rock check dams, temporary diversions, and temporary slope drains by linear feet installed and accepted.

Subsection 208.12 shall include the following:

# Pay Item Pay Unit

Silt Fence (Reinforced) (Special) Linear Foot