**REVISION OF SECTION 614**

### CONTROLLER CABINET FOUNDATION

**Section 614 of the Standard Specifications is hereby revised for this project as follows:**

**Section 614.10 (e) shall include the following:**

Controller foundations shall be preformed type and shall meet the following requirements:

Controller foundation shall be manufactured of fiberglass reinforced polymer concrete. Foundation dimensions shall conform to the detail in the plans. A minimum of 4 - ½ inch x 13 Unified Coarse Thread (UNC) inserts shall be installed for mounting of the controller cabinet to the foundation. Placement of the mounting inserts shall match the mounting configuration of the controller cabinet. The foundation shall be provided with an opening to accommodate access of underground conduit into the controller cabinet. Foundation opening shall match the controller cabinet opening as closely as possible. A minimum of 4 – ½ inch x 13 UNC lifting inserts shall be installed at each corner of the controller cabinet foundation. Lifting inserts shall be designed to support the full weight of the foundation to aid in the moving and placing of the foundation. The walking surface of the foundation shall have a skid resistant surface.

**Section 614.13, delete the nineteenth paragraph and replace with the following:**

Cabinets shall include pedestal and fiberglass reinforced polymer concrete foundations as required.