**REVISION OF SECTION 614**

**PEDESTRIAN PUSH BUTTON POST ASSEMBLY**

**Section 614 of the Standard Specifications is hereby revised for this project as follows:**

**Subsection 614.01 shall include the following:**

This work consists of the construction of a pedestrian push button and steel post assembly at locations as shown on the plans.

**Subsection 614.02 shall include the following:**

Post for pedestrian push button shall be tubular steel, Schedule 80.

Concrete for foundation shall be Class B.

Pedestrian push button and sign shall meet all ADA requirements.

Wiring for pedestrian push button shall conform to manufacturer recommendations.

**Subsection 614.03 shall include the following:**

Steel posts and slip base assembly shall be galvanized in accordance with Section 509, unless painting is called for on the plans. Painting shall be in accordance with Section 522, Duplex Coating System. The post and slip base shall be constructed as shown on the plans.

**Section 614.13 shall include the following:**

Pedestrian Push Button Post Assembly will be measured as the actual number that are installed and accepted.

**614.14 shall include the following:**

Pay Item Pay Unit

Pedestrian Push Button Post Assembly Each

Wiring will not be measured and paid for separately, but shall be included in the work.