**REVISION OF SECTION 630**

**IMPACT ATTENUATOR**

**(TRUCK MOUNTED ATTENUATOR)**

**Section 630 of the Standard Specifications is hereby revised for this project as follows:**

**In Subsection 630.01 shall include the following:**

This work shall consist of furnishing, operating, and maintaining a truck with a mounted attenuator.

**Subsection 630.09, shall include the following:**

*Truck Mounted Attenuator*. The Contractor shall supply a vehicle with a truck mounted attenuator approved by the FHWA to meet NCHRP 350 criteria for level TL-3 collisions. The attenuator shall be mounted to a suitable truck in a manner meeting the Manufacturer’s specifications. The truck shall also be furnished with a roof mounted Advance Warning Flashing or Sequencing Arrow Panel (B Type). The trucks may be used when setting up the work Zone and shall be parked in the activity area protecting the construction work when work begins.

**Subsection 630.13 shall include the following:**

Maintenance, storage, operation, and all repairs of Truck Mounted Attenuator and vehicle shall be the responsibility of the Contractor.

**Subsection 630.15 shall include the following:**

Truck Mounted Attenuators shall be measured by the Unit. The Contractor will be paid for the number of trucks required in the plans and available for use.

**Subsection 630.16 shall include the following:**

Pay Item Pay Unit

Impact Attenuator (Truck Mounted Attenuator) DAY

Payment will be full compensation for all labor, materials and equipment required to operate and maintain this truck for the duration of the project, including the attenuator and flashing panel.