October 21, 2010

REVISION OF SECTION 510

STRUCTURAL PLATE STRUCTURES

**NOTICE**

This is a standard special provision that revises or modifies CDOT’s *Standard Specifications for Road and Bridge Construction.* It has gone through a formal review and approval process and has been issued by CDOT’s Project Development Branch with formal instructions for its use on CDOT construction projects. It is to be used as written without change. Do not use modified versions of this special provision on CDOT construction projects, and do not use this special provision on CDOT projects in a manner other than that specified in the instructions unless such use is first approved by CDOT’s Standards and Specifications Unit. The instructions for use on CDOT construction projects appear below.

Other agencies which use the *Standard Specifications for Road and Bridge Construction* to administer construction projects may use this special provision as appropriate and at their own risk.

**Instructions for use on CDOT construction projects:**

Use in projects having steel plate or aluminum plate structures.

October 21, 2010

REVISION OF SECTION 510

STRUCTURAL PLATE STRUCTURES

Section 510 of the Standard Specifications is hereby revised for this project as follows:

In subsection 510.03 delete the third, fourth and fifth paragraphs and replace with the following:

All structural plates made from steel shall be made from plates formed and punched in accordance with Section 6 of AASHTO M 167.

All structural plates made from aluminum shall be made from plates formed and punched in accordance with Section 6 of AASHTO M 219.