MEMORANDUM

**DEPARTMENT OF TRANSPORTATION**

Project Development Branch

4201 East Arkansas Avenue

Denver, Colorado 80222

(303)757-9040

FAX (303)757-9868

**DATE**: April 26, 2012

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 105, Hot Mix Asphalt Pavement Smoothness

Effective this date, our unit is issuing a new standard special provision, Revision of Section 105, Hot Mix Asphalt Pavement Smoothness, dated April 26, 2012. This new standard special provision is 7 pages long. It should be used in projects having Hot Mix Asphalt (HMA), beginning with projects advertised on or after May 24, 2012. Please feel free, however, to include it projects advertised before this date.

This new standard special provision adds HRI Category III for roadways receiving a single layer of pavement that is being placed over an intermediate treatment or heating and scarifying. It also deletes the category for HRI percent improvement. The revised version of Design Bulletin 2011 Number 3, “Assigning Pavement Smoothness Categories”, should be used along with this special provision.

Those of you who keep books of Standard Special Provisions should add this new standard special provision to your file. For your convenience, we are attaching a new Index of Standard Special Provisions, which is also effective this date. In addition, you will find this and other special provisions that are being issued this date in one place in the CDOT Construction Specifications web site:

<http://www.coloradodot.info/business/designsupport/construction-specifications/2011-Specs>

Please click on the hyperlink titled “Recently Issued Special Provisions”.

LB/mrs

Attachments

Distribution: Per distribution list