MEMORANDUM

**DEPARTMENT OF TRANSPORTATION**

Project Development Branch, Standards and Specifications Unit

4201 East Arkansas Avenue

Denver, Colorado 80222

(303)757-9474

FAX (303)757-9820

**DATE**: January 30, 2014

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Section 206, Structure Backfill at Bridge Abutments

Effective this date, our unit is issuing a new Standard Special Provision, Revision of Section 206, Structure Backfill at Bridge Abutments. This new standard special is 1 page long, and should be used in projects having bridge construction. Use of this new Standard Special Provision is mandatory on projects advertised on or after February 27, 2014. You are free, however, to use it in projects advertised before this date.

This new standard special provision changes the default for backfill at bridge abutment to structure backfill (class 1) with mechanical reinforcement. Structure backfill (flow-fill) can still be used, when called for on the Plans.

Those of you who keep books of Standard Special Provisions should add this new Standard Special Provision to your file. The CDOT Construction Specifications web site has been updated to reflect the issuance of this and other special provisions. For your convenience, a new Index of Standard Special Provisions, dated January 30, 2014, is attached for your reference.

In addition, you will find this new standard special provision and other special provisions that have been issued effective this date in one place on the web site:

<http://www.coloradodot.info/business/designsupport/construction-specifications/2011-Specs/recently-issued-special-provisions>

If you have any questions or comments, please contact this office.

LB/ms

Attachments

Distribution: Per distribution list