

Standards and Specifications Unit

**Memorandum**

**DATE**: May 12, 2016

**TO**: All Holders of Standard Special Provisions

**FROM**: Larry Brinck, Standards and Specifications Engineer

**SUBJECT**: Revision of Sections 627 and 713 Modified Epoxy Pavement Marking

Effective this date, our unit is issuing a new standard special provision, Revision of Sections 627 and 713 Modified Epoxy Pavement Marking. This new standard special provision is 2 pages long.

Use this new standard special provision in projects having modified epoxy pavement marking, beginning with projects advertised on or after June 9, 2016. You are free to use this standard special provision in projects advertised before this date.

This new standard special provision replaces epoxy pavement marking with modified epoxy pavement marking, as the non-modified epoxy pavement marking is no longer in use in CDOT projects. It also upgrades application or coverage rates for glass beads in epoxy pavement marking.

Please note that because of this revision, the standard special provision, Revision of Section 713, Epoxy Pavement Marking, dated January 15, 2015, is hereby deleted.

Those of you who keep a book of Standard Special Provisions should add this new standard special provision to your file, and remove the obsoleted standard special provision described above. For your convenience, you can find this and others special provisions issued this date in one place at our Construction Specifications web page:

<https://www.codot.gov/business/designsupport/construction-specifications/2011-Specs>

Please scroll down and visit the hyperlink, “Recently Issued Special Provisions”.

If you have any questions or comments, please contact this office.