NOTICE

This Standard Special Provision (SSP) revises or modifies CDOT’s Standard Specifications for Road and Bridge Construction. These are the official instructions for its use on CDOT construction projects, and have been reviewed, approved, and issued by the Construction Engineering Services Branch. Use as written without change. Do not use modified versions of this SSP on CDOT construction projects. Do not use this special provision on CDOT projects in a manner other than specified in the instructions without approval by CDOT’s Standards and Specifications Unit. The instructions for use appear below.

Other agencies using the Standard Specifications for Road and Bridge Construction to administer construction projects may use this special provision appropriately and at their own risk.

**Instructions for use on CDOT construction projects:**

Use this standard special provision on all projects.

When identified on the Survey Tabulation sheet, all projects listed below

will apply:

1. All FHWA-assisted construction contracts.
2. All local agency FHWA-assisted contracts advertised on or after

August 1, 2022.

1. All state-funded CDOT construction contracts advertised on or

after August 1, 2022.

**Revise Section 625 of the Standard specifications as follows:**

**Add to Subsection 625.04, directly after the numbered list:**

The Contractor shall conduct an as-constructed survey of the following items: Installed or relocated utility lines as shown on the utility plans, including those installed or relocated by the Contractor or by others.

1. Installed or relocated culverts, conduit, inlets, or other drainage features.
2. Traffic signal heads, poles, pushbutton assemblies, and controller cabinets.
3. ITS fiber vaults, splice points, interfaces, nodes and other assets.
4. Lighting including pull boxes, meters and light standards.

The as-constructed survey shall be completed per the *CDOT Survey Manual*, Chapter 6, Section 6.14.