REVISION OF SECTION 611   
DEER GUARD

Section 611 is hereby added to the Standard Specifications for this project as follows:

**DESCRIPTION**

**611.01** This work consists of the construction of deer guards in accordance with these specifications and in conformity with the lines, grades, and details shown on the plans.

**MATERIALS**

**611.02** Concrete shall conform to the requirements of Section 601. Reinforcing steel shall conform to the requirements of Section 602. Structural steel shall conform to the requirements of Section 509. Timber shall conform to the requirements of Section 508. Fencing items shall conform to the requirements of Section 607.

**CONSTRUCTION REQUIREMENTS**

**611.03** Deer guards shall be constructed in accordance with the details shown on the plans. All work shall be done in accordance with the applicable construction methods contained in these specifications.

**METHOD OF MEASUREMENT**

**611.04** Deer guards will be measured by the number of units of the various sizes installed and accepted.

**BASIS OF PAYMENT**

**611.05** The accepted quantities of deer guards of the various sizes will be paid for at the contract unit price each when included in the bid schedule.

Payment will be made under**:**

**Pay Item Pay Unit**

\_\_\_\_ Foot Deer Guard Each