**REVISION OF SECTIONS 614 AND 713**

**SIGN PANEL (CLASS III)**

**Sections 614 and 713 of the Standard Specifications are hereby revised for this project as follows:**

**In subsection 614.04, delete the first paragraph and replace with the following:**

Sign panel materials shall conform to Section 713 and to the details shown on the plans. Retroreflective sheeting shall be Type XI as defined in the FHWA *Traffic Sign Retroreflective Sheeting Identification Guide*, and shall conform to subsections 713.04 and 713.06 when applicable.

**In subsection 713.06, delete the fourth paragraph and replace with the following:**

For all permanent signs, the legend, borders, and background shall be Type XI.

**Subsection 614.14 shall include the following:**

Pay Item Unit

Sign Panel (Class III) Square Foot