**REVISION OF SECTION 627**

**RESEARCH PROJECT PAVEMENT MARKING**

**Section 627 of the Standard Specifications is hereby revised for this project as follows:**

**Subsection 627.07 shall include the following:**

**627.07 *Research Project Pavement Markings.*** Research project pavement marking shall be installed per manufactures recommendations. Tyregrip, multipurpose high-friction surfacing by Prismo USA, Inc shall be used for installation where shown on the plans. Product to be used shall be approved for high vehicle traffic volumes (Annual Average Daily Traffic greater than 50,000) and severe weather durability. Marking Colors shall be as designated in the plans and/or approved by the Engineer.

**Subsection 627.12 shall include the following:**

High friction surfacing will not be measured but rather inspected for completed installation of the material.

**Subsection 627.13 shall include the following:**

**Pay Item** **Pay Unit**

Research Project Pavement Marking Lump Sum

Payment will be full compensation for all work necessary to complete this item including coordination.